|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bill Of Materials For System.DSN** | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| |  |  |  | | --- | --- | --- | | **Design Title** | : | System.DSN | | **Author** | : | Pham Van Thanh Tung | | **Revision** | : | TS.Pham Van Binh | | **Design Created** | : | Monday, September 21, 2009 | | **Design Last Modified** | : | Saturday, March 20, 2010 | | **Total Parts In Design** | : | 56 | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| 13 Resistors | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | Quantity: |  | References |  | Value |  | Order Code |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  | R1, R6->R8 |  | 10k |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 8 |  | R2->R4, R9->R13 |  | 1k |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | R5 |  | 10k |  | M10K |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| 8 Capacitors | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | Quantity: |  | References |  | Value |  | Order Code |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | C1 |  | 100u |  | Maplin KQ69A |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | C2 |  | 0.1u |  | Maplin KQ69A |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  | C3->C6 |  | 1u |  | Maplin VH03D |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 2 |  | C7, C8 |  | 33p |  | Maplin WX50E |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| 4 Integrated Circuits | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | Quantity: |  | References |  | Value |  | Order Code |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | U1 |  | ATMEGA32 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | U2 |  | 7805 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | U4 |  | MAX232 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | U5 |  | DS1307 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| 16 Diodes | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | Quantity: |  | References |  | Value |  | Order Code |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | D1 |  | 1N4372A  Zener 3.3v |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | D2 |  | 1N4731A  Zener 4.3 V |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 8 |  | D3->D8, D15, D16 |  | BAT46  normal Diodes |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 6 |  | D9->D14 |  | LED-YELLOW, Pin 2.54 mm |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| 16 Miscellaneous ( Cac Linh kien khac) | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | Quantity: |  | References |  | Value |  | Order Code |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  | B1->B4 |  | Buttons, 2.54 mm |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | J1 |  | 10073456-031LF  26 pins, 2 rows, 2.54 mm |  | FCI 10073456-031LF |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 1 |  | J2 |  | 10073456-001LF  10 pins, 2 rows, 2.54mm |  | FCI 10073456-001LF |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 4 |  | J3->J6 |  | 66226-010LF  10 pins, 1 row, 2.54mm |  | Digikey 609-2184-ND |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 2 |  | P1,P2 |  | COMPIM  Comport, 9 pins, female |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 2 |  | SW1, SW2 |  | SW-DIP4  (Cong Tac Dip 4) |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | 2 |  | X1, X2 |  | CRYSTALs  X1= 11.0592M  X2= 32.768kHz |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| *Saturday, March 20, 2010  11:58:49 PM* | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |